Drier Update Log

Drier_N32_V1.1.3
1.    Fix the problem that the humidity will display 99% when drying at high temperature(>110℃)

Drier_N32_V1.1.2
1.   Modify temperature and humidity iic protocol timing sequence

Drier_N32_V1.1.1
1.   Modify the minimum storage humidity to 10%
2.   Modify the incorrect French translation
3.  Calibrate the chamber heating power
4.   Add the factory mode

Drier_N32_V1.0.8
1.   First release