Creator4 Update log

creator4-221-VC518-20230804
1.   Fix the problem of abnormal printing temperature after pausing and changing filament during dual-color model printing with the litre cooling function enabled.
2.   Optimize the problem of abnormal extruder movement after resuming paused printing when in duplicate/mirror printing mode.
3.   Optimize the factory reset function. It will delete model files stored in the printer.
4.   Optimize the function of automatic shutdown after completing a print job.


creator4-219-VC518-20230411
1.   Enable the chamber light switch in the settings during printing.
2.   Optimize the protection mechanism of automatic shutdown under the condition of uncontrolled extruder heating.
3.   Fix the problem of incomplete printing of Cura and PrusaSlicer sliced files.
4.   Fix the problem that the extruder X-axis fails to home during auto leveling.
5.   Support printing dual-extruder models sliced by Cura.


creator4-216-VC517-20230315
1.   Add the mechanism of automatic repair after M3 upgrade fails.
2.   Fix abnormal problems occurred during XY-axis calibration.
3.   Fix other known bugs.


creator4-215-VC517-20230221
1.   Add the protection mechanism of automatic shutdown under the condition of uncontrolled extruder heating.
2.   Fix other known bugs.


creator4-214-VC515-20230209
1.   Update qt library files.
2.   Add the function of deleting temporary files when booting.                                                           

creator4-213-VC515-20230112
1.   Merge the firmware of single-motor and dual-motor versions.	
2.   Add instructions to enable the function of "heat preservation of the chamber before printing" in the slicing software.
3.   Fix the problem that it gets stuck at the video preview interface for a long time.
4.   Fix the problem of gaps occured in the models printed in the dual-color mode.
5.   Fix the occasional problem that it is unable to heat when chamber temperature enters the protection mode.
6.   Fix other known bugs.


creator4-177-407-434-20221025
1.   Add a maintenance tip popping up every 500 print hours.
2.   Modify the length of the Wi-Fi password that can be entered to be 30 digits.
3.   Turn off the power loss recovery command in the non-printing state.


creator4-176-407-434-20220921
1.   Fix the problem of abnormal sound when printing files in the mirror/duplicate mode with the leveling before printing function turned on.
2.   Fix some problems


creator4-175-407-434-20220801
1.   Optimize leveling and calibration		
2.   Add the temperature rise-and-fall function	
3.   Optimize the text of the filament change button
4.   Add the question mark key to the input keyboard
5.   Turn off the PCB fan during standby
6.   Able to connect to open Wi-Fi
7.   Update Korean translation
8.   Optimize the sensitivity of Y-axis current detection protection
9.   Remove the limit sensor detector during printing


creator4-169-407-430-20220420
1.   Add a prompt for insufficient capacity of the storage device.
2.   Add static IP settings.
3.   Increase the Z-axis calibration travel limit by 1mm.
4.   Modify the temperatures corresponding to each extruder: F-265℃, HT-320℃, HS-360℃.
5.   Fix the abnormal interface issue after the hotspot is frequently turned on and off.
6.   Fix the issue that the extruder hits the platform when long pressing the move button in the Z-axis calibration interface.


creator4-167-407-430-20220216
1.   The load/exchange speed and the clean speed of flexible filaments has been modified to 200mm/m
2.   The platform will drop 20mm when the auto-level fails
3.   Fix some bugs


creator4-166-407-430-20211216
1.   Fix the issue that in the mirror and duplicate mode, the printer will offset when resume printing after canceling right extruder printing.
2.   Fix the issue that it will trigger prompt multiple times when pressing the power button.
3.   Optimize filament detection, reduce false notification. 
4.   Optimize serial communication exception handling and program crash recovery.
5.   Add gcode files printing support.


creator4-164-407-422-20211122
1.   Add extruder cool down after printing pause due to lack of filament
2.   Add next print tips
3.   Add update log display
4.   Add Z coordinates display in Z axis calibration
5.   Add daemon
6.   Fix platform lift after printing
7.   Fix printing freeze
8.   Fix the wrong display range of real-time video
9.   Optimize auto calibration


creator4-161-407-422-20211028
1.   You can cancel one extruder in Duplication mode and mirror mode 
2.   Add machine name modify function		
3.   Update Chamber icon
4.   Set printer to busy status in calibration and auto level	
5.   Add video display		
6.   Fix Z coordinates error problem
7.   Fix layer display error after resume printing 			
8.   Modify Y limitation in manual interface		
9.   Modify minimum chamber and platform insulation time to 1 min		
10.   Fix printer stuck problem when the file is wrong
11.   Unify button color
12.   Optimize dual-color mode extruder switch movement


creator4-159-407-421-20211013
1.   Optimize printing pause fuction
2.   Fix flashprint camera cannot be open issue when network is unstable
3.   Set machine status to busy when changing filement, homing etc.
4.   Optimize ethernet interface
5.   Fix Flashcloud machine status issue
6.   Fix air filter after printing auto shutdown issue
7.   Update sdk file
8.   Fix wifi switch to hotspot issue
9.   Fix interface stuck when wifi list is null


creator4-157-407-418-20210929
1.   First release
